October 27, 2021

TMT Coordinated Chum Operation

Bonneville Dam Tailwater Operation for Chum Spawning 1

1. EFFECTIVE MONDAY, NOVEMBER 1, AT 0600 HOURS, AND UNTIL

FURTHER NOTICE, OPERATE THE BONNEVILLE DAM TAILWATER IN THE

FOLLOWING ORDER OF OPERATING RANGES AS PROJECT OUTFLOW INCREASES.

2. DURING ALL HOURS, OPERATE PROJECT OUTFLOW TO PROVIDE A

TAILWATER ELEVATION IN THE RANGE OF 11.3-13.0 FEET.

3. THEN, IF NECESSARY TO INCREASE PROJECT OUTFLOW, THE

TAILWATER MAY BE OPERATED UP TO 16.5 FEET DURING NIGHTTIME

HOURS (1700-0600). CONCENTRATE HIGHEST ELEVATIONS AROUND

2400 HOURS.

4. THEN, IF NECESSARY TO INCREASE PROJECT OUTFLOW, THE

TAILWATER MAY BE OPERATED UP TO 18.5 FEET DURING NIGHTTIME

HOURS (1700-0600).

5. THEN, IF INCREASING RIVER FLOW PRECLUDES THE ABILITY TO

MANAGE THE TAILWATER WITHIN THE STEPS ABOVE, OPERATE TO

PROVIDE A TAILWATER IN THE RANGE OF 13.0-16.5 FEET DURING

DAYTIME HOURS (0600-1700) AND UP TO THE MAXIMUM WITHIN

PROJECT 24-HOUR RAMP RATE LIMITS DURING NIGHTTIME HOURS

(1700-0600).