Table. Number of adult steelhead detections at two observation sites at Lower Granite Dam from September 01 – October 02 2022. Gray indicates when a total of 4 hours of spill 3 days / week and green indicates single 2 hour blocks 6 days/week.

|  |  |  |
| --- | --- | --- |
|  | Bypass (GRJ) | Spillway (GRS) |
| 1-Sep | 1 | 1 |
| 2-Sep | 2 |  |
| 3-Sep | 2 |  |
| 4-Sep | 2 | 1 |
| 5-Sep | 1 |  |
| 6-Sep | 2 | 1 |
| 7-Sep | 3 |  |
| 8-Sep | 1 | 1 |
| 9-Sep | 1 |  |
| 10-Sep |  |  |
| 11-Sep | 1 | 3 |
| 12-Sep |  |  |
| 13-Sep |  |  |
| 14-Sep |  |  |
| 15-Sep |  | 1 |
| 16-Sep |  |  |
| 17-Sep |  |  |
| 18-Sep |  | 3 |
| 19-Sep | 3 |  |
| 20-Sep |  | 3 |
| 21-Sep | 2 |  |
| 22-Sep | 1 | 4 |
| 23-Sep | 1 | 1 |
| 24-Sep | 4 |  |
| 25-Sep | 5 | 1 |
| 26-Sep | 1 |  |
| 27-Sep |  | 1 |
| 28-Sep | 1 |  |
| 29-Sep | 1 | 4 |
| 30-Sep | 1 | 1 |
| 1-Oct | 1 |  |
| 2-Oct | 2 |  |

Table. PIT detections at the LGR bypass (GRJ) and spillway (GRS) by hour September 01 – October 02 2022. Gray shows the general timing of split blocks of spill implemented before 22 September and Green shows timing of the 2 hour spill block after September 22.

|  |  |  |
| --- | --- | --- |
| Hour (PST) | Bypass (GRJ) | Spillway (GRS) |
| 0 | 2 |  |
| 1 | 1 |  |
| 2 | 1 |  |
| 3 | 1 |  |
| 4 | 4 |  |
| 5 |  | 4 |
| 6 | 1 | 7 |
| 7 | 1 | 6 |
| 8 | 2 | 5 |
| 9 | 1 | 4 |
| 10 | 2 |  |
| 11 | 3 |  |
| 13 | 4 |  |
| 14 | 1 |  |
| 15 | 3 |  |
| 16 | 3 |  |
| 17 | 1 |  |
| 18 | 2 |  |
| 20 | 3 |  |
| 21 | 1 |  |
| 23 | 2 |  |