October 19, 2022

TMT Coordinated Chum Operation

Bonneville Dam Tailwater Operation for Chum Spawning 1

1. EFFECTIVE TUESDAY, NOVEMBER 1, AT 0600 HOURS, AND UNTIL FURTHER

NOTICE, OPERATE THE BONNEVILLE DAM TAILWATER IN THE FOLLOWING

ORDER OF OPERATING RANGES AS PROJECT OUTFLOW INCREASES.

2. DURING ALL HOURS, OPERATE PROJECT OUTFLOW TO PROVIDE A TAILWATER

ELEVATION IN THE RANGE OF 11.3 - 13.0 FEET.

3. THEN, IF NECESSARY TO INCREASE PROJECT OUTFLOW, THE TAILWATER

MAY BE OPERATED UP TO 16.5 FEET DURING NIGHTTIME HOURS (1700-0600).

CONCENTRATE HIGHEST ELEVATIONS AROUND 2400 HOURS.

4. THEN, IF NECESSARY TO INCREASE PROJECT OUTFLOW, THE TAILWATER

MAY BE OPERATED UP TO 18.5 FEET DURING NIGHTTIME HOURS (1700-0600).

5. THEN, IF INCREASING RIVER FLOW PRECLUDES THE ABILITY TO MANAGE

THE TAILWATER WITHIN THE STEPS ABOVE, OPERATE TO PROVIDE A TAILWATER

IN THE RANGE OF 13.0-16.5 FEET DURING DAYTIME HOURS (0600-1700)

AND UP TO THE MAXIMUM WITHIN PROJECT 24-HOUR RAMP RATE LIMITS

DURING NIGHTTIME HOURS (1700-0600).