**THE DALLES FISHWAY DEWATER SCHEDULE**

**2022-23**

Operate AWS with 1 fish unit Debris management PDT Nov 24-Dec1

FU1, FU2 and AWS OOS ROV inspect intakes Dec1

East Fishladder Dewater Dec 6, 2022

1. 155 repair
2. 154 and 155 lamprey orifice cut
3. Inspect lower ladder grating
4. Scan for PITs (TDF)
5. ROV exit trashrack inspect
6. Install exit oil boom

East Fishway below tailwater ROV Dec ?, 2022

1. Inspect grating

North Fishladder Dewater Jan 9, 2023

1. Inspect diffuser valve at count station
2. Pull Exit trashrack inspect
3. Pull PUD intake trashrack inspect
4. Remove more vegetation

North Fishway below tailwater ROV Jan ?, 2023

1. Inspect grating
2. Finish SCADA north entrance

Ice Trash Sluiceway OOS Dec 16, 2022

1. Endgate inspect
2. Lower channel check for spalling

\*Return date for each fishway dependent on work completion.

\*One fishway out of service at a time.

\*Apply full flushing overnight after EFL dewater and fish