**CENWP-ODJ8/30/2024**

**MEMORANDUM FOR THE RECORD**

**SUBJECT: *24JDA13 Spillway Crane OOS and Unable to Close TSW-18***

On 29 August 2024 at approximately 1400, the JDA spillway crane went out of service due to a transformer failure. Unfortunately, there isn’t a replacement part onsite, and due to the specifics of the part, it may be difficult to replace. Crews were able to close the TSW in spillbay-19 but were unable to close the TSW in spillbay-18. There is no other way to close the TSW, as using a mobile crane would be unsafe.

In order to maintain the FPP spill requirement of 20-KCFS, spillways 2, 3, 4, and TSW-18 was open until 1 September 2024. Starting 1 September 2024 only spillway 2 will be open with the TSW, and total spill will be approximately 10-12 KCFS. Operations will continue to utilize the TWS open unit priority table until the TSW can be removed and the spillway gate is closed.

1. Species – NA
2. Origin – NA
3. Length – NA
4. Marks and tags – NA
5. Marks and Injuries found on carcass – NA
6. Cause and Time of Death – NA
7. Future and Preventative Measures- NA

Sincerely,

Project Fisheries