**OFFICIAL COORDINATION REQUEST FOR**

**NON-ROUTINE OPERATIONS AND MAINTENANCE**

**COORDINATION TITLE –** 16BLU04 Spillway Gate Repair

**COORDINATION DATE –** 16 June 2016

**PROJECT –** Blue River Dam

**RESPONSE DATE –** 30 June 2016

**Description of the problem**

To ensure Blue River Dam can fully perform its mission helping reduce flood damage to Willamette River communities, the WVP will be rehabilitating the dam’s two spillway gates.

The rehabilitation of the gates requires the work area remain dewatered. Blue River Dam’s reservoir will be managed to keep the elevation below 1,301 feet, about 20 feet below the spillway crest.

**Type of outage required**

Spillway gates will not be available during the construction windows.

**Impact on facility operation**

No spill capabilities at Blue River Dam during the construction windows.

**Dates of impacts/repairs**

Gate 1: Sep 15-Nov 15 2016

Gate 2: Sep 15-Nov 15, 2017

**Length of time for repairs**

It is estimated spillway gate repairs will require about eight weeks for each gate.

**Expected impacts on fish**

There will be no observable impacts to fish.

**Comments from agencies**

**Final results**

Please email or call with questions or concerns.

Thank you,

Chris Walker

U.S. Army Corps of Engineers

NWP Operations Division Fish Section

Willamette Operations Coordination Biologist

503.808.4316

Christopher.E.Walker@usace.army.mil