# Fish Passage Plan (FPP) Change Request Form

**Change Form # & Title**: 21LMN004 – RSW Criteria

**Date Submitted**: 4 January 2021

**Project**: Lower Monumental

**Requester Name, Agency**: Lisa Wright, Corps RCC

**Final Action: APPROVED – 28 January 2021**

**FPP Section**: LMN section 2.3.2.6. RSW

**Justification for Change**: Updates RSW operating criteria to include spill for steelhead. Also clarifies that the estimated RSW spill rate is based on the forebay in MOP. At higher forebay elevations, more water would be spilled over the RSW.

**Proposed Change**:

**2.3.2.6. Removable Spillway Weir (RSW).**

Lower Monumental Dam has one removable spillway weir (RSW) that provides a surface passage route via spillbay 8. The RSW is opened and closed from the control room and spills approximately 6.8 kcfs when the forebay elevation is in the MOP range.

The RSW will be in the raised position and operational during spill for juvenile fish passage (**Appendix E**)and during spill for adult steelhead (**section 2.2**). Raise the spill gate to where it does not touch flow passing down the RSW.

**Comments**:

**Record of Final Action**: Approved at the FPOM FPP meeting on 28-JAN-2021.