# Fish Passage Plan (FPP) Change Form

**Change Form # & Title**: 22JDA006 – Ladder Temperature Dates

**Date Submitted**: 9-November-2021

**Project**: John Day Dam

**Requester Name, Agency**: Scott Fielding, Michael Lotspeich, Laura Ricketts CENWP-ODJ

**Final Action: APPROVED 27-January-2022**

**FPP Section**: JDA section 2.4.2.11.b. Fishway Temperature Monitoring.

**Justification for Change**: On the FPC website it states, “Hourly adult ladder water temperatures are graphed from April 1 through October 31st.”

**Proposed Change**: *Edits to existing FPP text in “track changes”.*

**2.4.2.11.b.** From ~~June 1 through September 30~~ April 1 through October 31, measure water temperature at adult fishway entrances and exits and submit data to the Fish Passage Center (FPC) weekly for posting online. Ensure the location of the monitors meets the following criteria:

Within 10 meters of all shore-oriented entrances and exits.

Entrance monitor within 1 meter above the ladder floor and at least 10 meters downstream of ladder diffusers, if possible, to allow for sufficient mixing with surface water.

Exit monitor within 1 meter above the ladder floor and above all diffusers to allow for sufficient mixing with surface water.

If an existing temperature monitoring location is proposed to be used for either the exit or entrance, verify that the site accurately reflects water temperature within 10 meters of the entrance or exit.

**Comments**:

**Record of Final Action**: Approved at the FPOM FPP meeting 1/27/22.