# Fish Passage Plan (FPP) Change Form

**Change Form # & Title**: 22TDA005 – 2.3.2.7. Orifice Blocker Install Time

**Date Submitted**: 29-December-2021

**Project**: The Dalles Dam

**Requester Name, Agency**: Bob Cordie, Corps TDA

**Final Action: APPROVED 27-January-2022**

**FPP Section**: TDA section 2.3.2. Juvenile Facilities / Fish Passage Season

**Justification for Change**: Install time is longer than 1 hour due to safety clearance logistics and realistic time for operational adjustments.

**Proposed Change**:

Change 1 hour to 5 hours.

**2.3.2. Juvenile Fish Facilities – Juvenile Fish Passage Season (April 1 – November 30).**

**2.3.2.7.** When units are being dewatered, leave ITS endgate open and close sluice gates to expose gatewell orifices, then install orifice blocker. After orifice-sealing devices are installed, sluice gates should be returned to the open position. All 6” orifices will be closed as units are dewatered. Installation time should be approximately 5 hours.

**Comments**:

1/27/22 FPOM FPP Meeting:

Lorz, Bellerud – fine with this. Van Dyke - again concerned with why the need for more time? What's changed? Cordie - this has been outdated for a while. Clearance programs have gotten more complicated and time consuming to ensure safety.

**Record of Final Action**: Approved at FPOM FPP meeting 1/27/22.