**High Head Dams with Collectors**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Dam** | **Owner** | **Date**  **Installed** | **Target Species** | **Collection Efficiency** |
| Upper Baker Dam | PSE | 2008 | Coho  Sockeye | 83% - 99%  84% - 96% |
| Lower Baker Dam | PSE | 2013 | Coho  Sockeye | 93% - 95%  92% |
| Cushman Dam | TAC | 2015 | Coho | 33% to 36% |
| Swift Dam | PAC | 2012 | Steelhead  Coho  Chinook | 19% to 25%  12% to 31%  11% |
| Round-Butte | PGE/WST | 2009 | Steelhead  Chinook | 5% to 48%  7% to 65% |

**Run of River Dams with Collectors**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Dam** | **Owner** | **Date**  **Installed** | **Target Species** | **Collection Efficiency** |
| North Fork | PGE | 2012 | Steelhead  Coho | 91% to 96%  75% to 96% |
| River Mill | PGE | 2015 | Steelhead  Coho  Chinook | 97%  99%  96% |