# Fish Passage Plan (FPP) Change Request Form

**Change Form # & Title**: 17TDA005 –Sluiceway Operation during Involuntary Spill

**Date Submitted**: March 9, 2017

**Project**: TDA

**Requester Name, Agency**: Bob Cordie, The Dalles Fisheries

**Final Action:** **APPROVED as Revised Mach 9, 2017**

**FPP SECTION**: TDA 2.2.2. Spill Management.

**JUSTIFICATION**: No specification as to how many gates.

**PROPOSED CHANGE**: (edits to existing FPP text shown in “track changes”)

**2.2.2.** During spill that occurs December 16 through the end of February, the Ice & Trash Sluiceway (ITS) will be operated if available to provide a surface passage route. Operate 3 gates on Unit 1 and 3 gates on Unit 18.

Table TDA-4. The Dalles Dam Ice & Trash Sluiceway (ITS) Schedule of Operations.

|  |  |  |  |
| --- | --- | --- | --- |
| **DATES** | **SLUICEWAY OPERATION (24 hrs/day)** | **PURPOSE** | **FPP Section** |
| March 1–31; December 1–15 | OPEN End gate  OPEN Sluice gates 1-2, 1-3 / 18-1, 18-2 | Adult fallback; kelt passage | 2.4.1.6;  2.4.2.9 |
| April 1–  November 30 | OPEN End gate  OPEN Sluice gates 1-1, 1-2, 1-3 / 8-2, 8-3 / 18-2 | Juvenile passage | 2.3.2.5 |
| \*December 16–  end of February | \*CLOSE End gate  OPEN Sluice gates 1-1 / 18-3 | \*No passage; allows egress when equalized w/forebay | 2.3.1.6, 2.4.1.6 |

\*Except during periods of spill when the ITS will be operated if available, as defined in **section 2.2.2** (3 gates on Unit 1 and 3 gates on Unit 18).

**COMMENTS**:

3/9/17: FPOM requested also adding this info to Table TDA-4.

**RECORD OF FINAL ACTION**: APPROVED as revised at FPOM 3/9/17