# Fish Passage Plan (FPP) Change Request Form

**Change Form # & Title**: 21AppB003 – Additional transport truck

**Date Submitted**: July 1, 2021

**Project**: Lower Granite Dam

**Requester Name, Agency**: Scott St. John, USACE - NWW

**Final Action**: **APPROVED – July 8, 2021**

**FPP Section**: Appendix B section 4.5.4 and 5.1.1.

**Justification for change**: The USACE has purchased a 1,000 gallon slide on tank and truck to add to the Juvenile Fish Transportation Program equipment.

**Proposed Change**: Changes are proposed for two sections:

1. Subsection 4.5.4 updated Table B (see below).

Table B-1. Juvenile Fish Transportation Program Transport Vehicle Capacity.

| **Transport Vehicle** | **Capacity (gal)** | **Inflow (gpm)** | **Fish Capacity (lbs)** |
| --- | --- | --- | --- |
| Barge 2127 - “*SOCKEYE*” | 85,000 | 4,600 | 23,000 |
| Barge 2817 - “*BLUEBACK*” | 85,000 | 4,600 | 23,000 |
| Barge 4382 - “*STEELHEAD*” | 100,000 | 10,000 | 50,000 |
| Barge 4394 - “*COHO*” | 100,000 | 10,000 | 50,000 |
| Barge 8105 - “*CHINOOK*” | 150,000 | 15,000 | 75,000 |
| Barge 8106 - “*KING* *SALMON*” | 150,000 | 15,000 | 75,000 |
| Barge 8107 | 150,000 | 15,000 | 75,000 |
| Barge 8108 | 150,000 | 15,000 | 75,000 |
| Truck | 3,500 | n/a | 1,750 |
| Truck-Slide on tank | 1,000 | n/a | 500 |
| Truck-Slide on tank | 750 | n/a | 375 |
| Truck - Midi-tank | 300 | n/a | 150 |
| Truck - Mini-tank | 150 | n/a | 75 |

1. Section 5.1.1 See added text below

**5.1.1 Trucks.** Two 3,500-gallon fish transport trailers and one tractor, one 1000-gallon tank, one 750-gallon tank, three 300-gallon midi-tanks, and three 150-gallon mini-tanks are available for hauling fish. One midi-tank and one mini-tank will be provided at each Snake River collector project. Mini- and midi-tanks are small units that can be mounted onto pickup trucks. During trucking operations, a transport truck/trailer is based at Lower Granite Dam, with the second transport trailer held in reserve. In addition, a 1000-gallon tank and truck is based at Lower Granite Dam and a 750-gallon tank and truck is based at Little Goose Dam. The truck/trailer combination may be redistributed to meet transport demands and when smaller transport vehicles begin operating in late summer.

**Comments**:

**Record of Final Action**: Approved at the FPOM meeting on July 8, 2021.