# Fish Passage Plan (FPP) Change Form

**Change Form # & Title**: 22TDA002 – 2.3.1.3. Spill Gate Maintenance Dates

**Date Submitted**: 29-December-2021

**Project**: The Dalles Dam

**Requester Name, Agency**: Bob Cordie, Corps TDA

**Final Action: APPROVED 27-January-20200**

**FPP Section**: TDA section 2.3.1. Juvenile Facilities / Winter Maintenance Period

**Justification for Change**:

Spillway maintenance usually start in October. Maintenance work should be allowed anytime outside the spill season.

**Proposed Change**:

**2.3.2. Juvenile Fish Facilities - Winter Maintenance Period (December 1 – March 31).**

**2.3.1.3.** Inspect and repair spill gates and control systems where necessary. The spillway must be able to achieve spill patterns on April 10 through August 31, except for coordinated changes. No more than two functioning bays within the spillwall may be out at one time in case of spill.

**Comments**:

1/27/22 FPOM FPP Meeting:

Lorz – add language to specify how many bays out at one time within the spillwall to ensure they have capacity to spill if necessary.

Cordie – ok with saying no more than two bays at a time.

**Record of Final Action**: Approved as revised at the FPOM FPP meeting 1/27/22